> # RMON Thresholds Controls

> Field | Description
> --- | ---
> AlarmEnable | If true, the RMON alarm feature is enabled. If the RMON feature is disabled, all the RMON alarm related polling are stopped. Note that this is only intended for temporary disabling of RMON alarm feature to ensure that the CPU usage by RMON alarms is not detrimental. For permanent disabling on this feature, it suggested that all the entries in the alarmTable are removed.
> MaxAlarms | The maximum number of entries allowed in the alarmTable.

> Related Topics

> RMON Alarm Configuration Information

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.