> # Configuring Fibre Channel Routes

> ## Detailed Steps

> If you disable FSPF, you can manually configure a Fibre Channel route.

> To configure a Fibre Channel route using Device Manager, follow these steps:

> 1. Click FC > Advanced > Routes.

> You see the FC Static Route Configuration dialog box.

> 2. Click Create to create a static route.

> You see the Create Route dialog box.

> 3. Select the VSAN ID that you are configuring this route.
> 4. Fill in the destination address and destination mask for the device you are configuring a route.
> 5. Select the interface that you want to use to reach this destination.
> 6. Select the next hop domain ID and route metric.
> 7. Select either the local or remote radio button.
> 8. Click Create to save these changes or click Close to discard any unsaved changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.