> # CDP Neighbors

> Field | Description
> --- | ---
> Switch | The Internet address for this entity.
> Local Interface | A unique value that identifies the interface on this FCIP device to which this link pertains.
> DeviceName | The remote device's name. By convention, it is the device's fully qualified domain name.
> DeviceID | The device ID string as reported in the most recent CDP message.
> DevicePlatform | The version string as reported in the most recent CDP message.
> Interface | The port ID string as reported in the most recent CDP message.
> IPAddress | The (first) network-layer address of the device's SNMP-agent as reported in the address TLV of the most recently received CDP message.
> NativeVLAN | The remote device's interface's native VLAN, as reported in the most recent CDP message. The value 0 indicates no native VLAN field (TLV) was reported in the most recent CDP message.
> PrimaryMgmtAddr | Indicates the (first) network layer address at which the device will accept SNMP messages as reported in the most recently received CDP message.
> SecondaryMgmtAddr | Indicates the alternate network layer address at which the device will accept SNMP messages as reported in the most recently received CDP message.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.