> # Enabling Dynamic Mapping

> ## Detailed Steps

> To enable dynamic mapping of Fibre Channel targets into iSCSI using Device Manager, follow these steps:

> 1. Choose IP > iSCSI.
> - You see the iSCSI configuration.
> 2. Click the Target tab to display a list of existing iSCSI targets.
> 3. Check the Dynamically Import FC Targets check box.
> 4. Click Apply to save this change.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.