Viewing the Status of the Tape Device

Use the show sme internal info cluster <cname> tape-all command to view tape information.

SWitch# show sme internal info cluster tie1 tape-all

Tape Backup Groups : 1

Last Seq Id : 1

Tape Backup Group : tb2

Memory Address : 0x10788854

Seq Id : 1

Compression : Enabled

Key on Tape : Disabled

Tape Key Recycle : Enabled

Shared Key Mode : Disabled

Auto Volume Group : Disabled

Tape Devices : 1

Last Device Seq Id : 4

Tape Volgrps : 1

Last Volgrp Seq Id : 1

Tape Devices : 1

Last Seq Id : 4

Tape Device : td0

Memory Address : 0x107ba054

Seq ID : 4

SME (Encryption) : Enabled

Compression : Enabled

Bypass-Policy : BYPASS DISABLED

Cached Lun Path : (nil)

FSM State : SME_CTAPE_DEVICE_G_ST_STABLE

ITL Count : 1

Tape Drive : 0x107d123c

LUN FSM State : SME_LUN_ST_STABLE

Lun Path :0x107d185c

IT :V 3 I 40:00:00:00:00:00:00:01 T 40:00:00:00:00:00:00:02

LUN :0x0000

Is Configured

Status :2

Error :0x0

Flags :0x1

Use the sh sme internal info cluster tie1 tape-bkgrp tb2 tape-device td0 to view the information about a particular Tape Device in a particular Tape Backup Group.

Switch# sh sme internal info cluster tie1 tape-bkgrp tb2 tape-device td0

Tape Device : td0

Memory Address : 0x107ba054

Seq ID : 4

SME (Encryption) : Enabled

Compression : Enabled

Bypass-Policy : BYPASS DISABLED

Cached Lun Path : (nil)

FSM State : SME_CTAPE_DEVICE_G_ST_STABLE

ITL Count : 1

Tape Drive : 0x107d123c

LUN FSM State : SME_LUN_ST_STABLE

Lun Path :0x107d185c

IT :V 3 I 40:00:00:00:00:00:00:01 T 40:00:00:00:00:00:00:02

LUN :0x0000

Is Configured

Status :2

Error :0x0

Flags :0x1

Use the Show Interface smex/y to view statistical information about the SME interface configured for Encryption.

Switch# sh int sme1/1

sme1/1 is up

In fabric Fabric_sw119

Member of cluster tie1

SME IOs IO/s Bytes Rate

----------------------------------------------------------------------------

Host Reads 0 0 0 0.00 B/s

Host Writes 0 0 0 0.00 B/s

Host Total 0 0 0 0.00 B/s

Tgt Reads 0 0 0 0.00 B/s

Tgt Writes 0 0 0 0.00 B/s

Tgt Total 0 0 0 0.00 B/s

Clear IOs IO/s Bytes Rate

----------------------------------------------------------------------------

Host Reads 0 0 0 0.00 B/s

Host Writes 0 0 0 0.00 B/s

Host Total 0 0 0 0.00 B/s

Tgt Reads 0 0 0 0.00 B/s

Tgt Writes 0 0 0 0.00 B/s

Tgt Total 0 0 0 0.00 B/s

Compression Ratio 0 : 0

SME to Clear 0.00 %

Read to Write 0.00 %

Clear Luns 1, Encrypted Luns 0

Error Statistics

0 CTH, 0 Authentication 0 Compression

0 Key Generation, 0 Incorrect Read Size

0 Overlap Commands, 0 Stale Key Accesses

0 Overload Condition, 0 Incompressible

0 XIPC Task Lookup, 0 Invalid CDB

0 Ili, 0 Eom, 0 Filemark, 0 Other

2 FAILED WRITE Count - BYPASS DISABLED by USER ======> If write fails for clear text tape

last error at Tue Jun 26 13:39:49 2012

Use the module Commands to view LUN specific information.

show sme internal info crypto-node 1 lun all

module-1# sh sme internal info crypto-node 1 lun all

TAPE LUN TREE

LUN

---

cpp_lun_ndx 0x5

serial no. 0003-0000-00000000:0000000000000000

type sequential

sme_enabled 1

crypto_status 0

vendor_id SONY

product_id SDZ-130

asl_id

prod_rev_level 0201

vendor_specific

cluster_name tie1

enable_pad False

pad to 0x0

bkgrp_name tb2

device_name td0

flags 0

granularity 2

max_block_len_lim 1000

min_block_len_lim 4

block_length 512

compression 1

key_ontape 0

Bypass_Policy BYPASS DISABLED

has tape yes

position 200

has cth no

bypass enc no

wrap guid 0000000000000000-0000000000000000

media guid 0000000000000000-0000000000000000

total itl count 1

active itl count 1

cmd_send_err 0

Not locked