> # LUN Discover

> Field | Description
> --- | ---
> StartDiscovery | If Local, then only the directly attached SCSI target devices/ports and LUNs associated with them on all VSANs will be discovered. If Remote, then all SCSI target devices/ports and LUNs associated with them on all VSANs in the whole fabric, except the directly attached ones, will be discovered.
> Type | Selecting targets results in only targets being discovered, without the NS results in both targets and LUNs being discovered.
> OS | Specifies the operating system on which the LUNs need to be discovered.
> Status | Indicates the outcome of the LUN discovery on the local switch. Contains the status of the most recent discovery. inProgress(1) - indicates that the discovery is still in progress. completed(2) - indicates that the discovery is complete. failure(3) - indicates that the discovery encountered a failure.
> CompleteTime | When the last discovery was completed. The value will be zero or N/A, if discovery has not been performed since the last system restart.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.