> # Preferred Path Maps Active

> Field | Description
> --- | ---
> VSAN Id, Route Id, Preference | The VSAN ID of this FC route map. An arbitrary integer value that identifies a route in this FC route map. Preference level, which indicates the metric or cost.
> Interface | Represents an interface on the local device on which the matched or classified frame will be forwarded.
> IVR Nexthop VSAN | Represents the IVR next hop VSAN ID.
> Selected ? | The status of the indexed set entry.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.