> # Event Filters General

> Field | Description
> --- | ---
> FSPF - Nbr State Changes | Specifies whether or not the local switch should issue notification when the local switch learns of a change in the neighbor's state (state in the FSPF neighbor finite state machine) on an interface on a VSAN.
> Domain Mgr - ReConfig Fabrics | Specifies whether or not the local switch should issue a notification on sending or receiving ReConfigureFabric (RCF) on a VSAN.
> Zone Server - Request Rejects | Specifies if the zone server should issue a notification on rejects.
> Zone Server - Merge Failures | Specifies if the zone server should issue a notification on merge failures.
> Zone Server - Merge Successes | Specifies if the zone server should issue a notification on merge successes.
> Zone Server - Default Zone Behavior Change | Specifies if the zone server should issue a notification if the propagation policy changes.
> Zone Server - Unsupp Mode | Specifies if the zone server should issue a notification on unsupp mode changes
> FabricConfigServer - Request Rejects | Specifies if the fabric configuration server should issue a notification on rejects.
> RSCN - ILS Request Rejects | Specifies if the RSCN module should generate notifications when a SW_RSCN request is rejected.
> RSCN - ILS RxRequest Rejects | Specifies if the RSCN module should generate notifications when a SW_RSCN request is rejected.
> RSCN - ELS Request Rejects | Specifies if the RSCN module should generate notifications when a SCR or RSCN request is rejected.
> FRU Changes | A false value will prevent field replaceable unit (FRU) notifications from being generated by this system.
> SNMP - Community Auth Failure | Indicates whether the SNMP entity is permitted to generate authenticationFailure traps.
> VRRP | Indicates whether the VRRP-enabled router will generate SNMP traps for events defined in this MIB.
> FDMI | Specifies if the FDMI should generate notifications when a registration request is rejected.
> License Manager | Indicates whether the system should generate notifications.
> Port/Fabric Security | Specifies if the system should generate notifications when a port/fabric security issue arises.
> FCC | Specifies whether the agent should generate notifications.
> Name Server | If checked, the name server generates a notification when a request is rejected. If false, the notification is not generated.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.