> # Default Settings

> Table 9-4 lists the default settings for trunking parameters.

> Table 9-4 Default Trunk Configuration Parameters
> Parameters | Default
> --- | ---
> Switch port trunk mode | ON on non-NPV and MDS core switches. OFF on NPV switches.
> Allowed VSAN list | 1 to 4093 user-defined VSAN IDs.
> Allowed VF-ID list | 1 to 4093 user-defined VF-IDs.
> Trunking protocol on E ports | Enabled.
> Trunking protocol on F ports | Disabled.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.