> # Call Home Alerts

> Field | Description
> --- | ---
> Action | Test — Sends a Call Home message TestWithInventory — Sends a message with inventory details.
> Status | The status of the last Call Home action invocation.
> FailureCause | The failure cause for the last Call Home test invocation.
> LastTimeSent | When the last Call Home alert was sent.
> NumberSent | The number of Call Home alerts sent.
> Interval | Time frame for sending the periodic software inventory Call Home message.
> Throttling Enable | If checked, enables the message throttling mechanism implemented on the system, to limit the number of Call Home messages for an alert type within a time frame. The maximum is 30 in a 2-hour time frame, and any further messages for that alert type are discarded.
> Enable | If checked, enables the sending of periodic software inventory Call Home messages on the system.

> Related Topics

> Call Home Alert Groups

> Customizing Alert Group Messages

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.