> # Configuring the Default Zone Policy

> ## Detailed Steps

> To permit or deny traffic in the default zone, follow these steps:

> 1. Choose Zone > Edit Local Full Zone Database.

> You see the Select VSAN dialog box.

> 2. Select a VSAN and click OK.

> You see the Edit Local Full Zone Database dialog box for the selected VSAN.

> 3. Choose Edit > Edit Default Zone Attributes to configure the default zone QoS priority attributes.

> You see the Modify Default Zone Properties dialog box.

> 4. Set the Policy drop-down menu to permit to permit traffic in the default zone, or set it to deny to block traffic in the default zone.
> 5. Click OK to save these changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.