> # Bandwidth Reservation: 32-Port 256-Gbps Advanced Fibre Channel Module

> RateMode Configuration Macro | Description
> --- | ---
> Dedicated 8 Gbps on all ports — initial and default settings | Allocates a rate mode of 8 Gbps on all the available ports.
> Shared 8 Gbps on all ports—initial and default settings | Allocates a rate mode of shared 8 Gbps on all the available ports.
> Dedicated 10 Gbps on following ports: 2, 3, 4, 5, 6, 8 (ports 1 and 7 disabled) 10, 11, 12, 13, 14, 16 (ports 9 and 15 disabled) 18, 19, 20, 21, 22, 24 (ports 17 and 23 disabled) 26, 27, 28, 29, 30, 32 (ports 25 and 31 disabled) | Allocates a rate mode of 10Gbps on the following ports.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.