## Choosing High Availability Settings

Detailed Steps

To choose the primary or secondary server, follow these steps:

1. From DCNM-SAN Web Client, choose Key Manager Settings.

2. In the High Availability Settings area, click Edit HA Settings.

3. Choose the KMC role of the server to be the Primary Server and specify the IP address of the SME Secondary KMC. Alternately, you can choose the server to be the secondary server and specify the IP address of the primary server.

4. Click OK to save the settings to view the notification that the settings have been saved.