> # Analyzing a Zone Merge

> ## Detailed Steps

> To perform a zone merge analysis, follow these steps:

> 1. Choose Zone > Merge Analysis.

> You see the Zone Merge Analysis dialog box.

> 2. Select the first switch to be analyzed from the Check Switch 1 drop-down list.
> 3. Select the second switch to be analyzed from the And Switch 2 drop-down list.
> 4. Enter the VSAN ID where the zone set merge failure occurred in the For Active Zoneset Merge Problems in VSAN Id field.
> 5. Click Analyze to analyze the zone merge.
> 6. Click Clear to clear the analysis data in the Zone Merge Analysis dialog box.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.