> # Port Tracking Force Shut

> Field | Description
> --- | ---
> Interface | The interface of the port to be configured for the forced-shut mode.
> Force Shut | If true, the port is brought down administratively, and you must bring the port up manually. If false, the port is brought down operationally only, and is brought up again as soon as any one of the tracked ports comes up.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.