> # IVR Action

> Field | Description
> --- | ---
> Activate Local Topology | Setting this object to activate is a request for the configured IVR topology to be activated on this device. i.e., for the current configuration of IVR topology to be cloned, with the clone becoming the active IVR topology.
> IsActive | This object indicates of IVR topology is active or not. If true, the IVR topology is active. If false, the IVR topology is not active.
> Activation Time | When the IVR topology was most recently activated. If the IVR topology has not been activated prior to the last re-initialization of the local network management system, then this value will be N/A.
> Enable IVR NAT | Enable FCID and VSAN identifier translation across VSAN boundaries. If true, the VSAN identifier as well as the entire FCID of the end devices would be modified as frames cross VSAN boundaries.
> Auto Discover Topology | Enable automatic VSAN topology discovery. If true, automatic VSAN topology discovery is turned on. IVR processes would communicate with each other to provide a global view of the physical topology to all the IVR enabled switches. If false, automatic VSAN topology discovery is turned off.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.