> # Modules - Status and Config

> Field | Description
> --- | ---
> Name | Module description.
> Module | Module name identifier.
> OperStatus | Module's operational state.
> Reset | Click to reboot the module.
> RateModeOverSubscription Limit | Select this option to control the restriction on the oversubscription ratio on modules that support it. By default, the restriction is enabled. If you disable this option, all the interfaces on the module are capable of operating at maximum admin speed, regardless of the available bandwidth.
> BandwidthFairnessConfig | Select this option to control bandwidth fairness on modules that support it. By default, bandwidth fairness is enabled.
> BandwidthFairnessOper | Shows if bandwidth fairness is enabled or disabled. By default, bandwidth fairness is enabled.
> X2 xcvrFrequency Config | Specifies the transceiver frequency of the module. notApplicable - Select this when the module does not support this configuration. xcvrFreqX2FC - Select this to set the module’s FC transceiver frequency to10 Gigabyte. xcvrFreqX2Eth - Select this to set the module’s Ethernet transceiver frequency to10 Gigabyte.
> ResetReasonDescription | Why module was last reset.
> Local Switching Mode | Shows the status of the local switching modules.
> StatusLastChangeTime | When OperStatus was changed.
> Power Admin | Allows you to power on and off the Field Replaceable Unit (FRU).
> Power Oper | Field Replaceable Unit (FRU) operational power state.
> Current | Current supplied by the Field Replaceable Unit (FRU).

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.