> # Configuring the Drop Latency Time

> You can change the default latency time for a network, a specified VSAN in a network, or for the entire switch.

> ## Detailed Steps

> To configure the drop latency time for a switch, follow these steps:

> 1. Expand a fabric and select All VSANS.

> You see the VSAN configuration in the Information pane.

> 2. Click the Attributes tab.

> You see the general VSAN attributes in the Information pane.

> 3. Double-click the Network Latency field and change the value.
> 4. Click Apply Changes to save these changes, or click Undo Changes to discard any unsaved changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.