> # Ethernet PortChannels

> Field | Description
> --- | ---
> Description | Alias name for the interface as specified by a network manager.
> Members | Members of this Ethernet port channel.
> Oper Speed | Operational speed of the interface.
> Mtu | The size of the largest frame which can be sent/received on the interface, specified in bytes.
> PhysAddress | The interface's MAC address.
> Status Admin | The desired state of the interface.
> Status Oper | The current operational state of the interface.
> LastChange | When the interface entered its current operational state. If the current state was entered prior to the last re-initialization of the local network management subsystem, then this value is N/A.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.