> # Configuring a CRL

> ## Detailed Steps

> To configure the CRL from a file to a trust point, follow these steps:

> 1. Click Switches > Security > PKI in the Physical Attributes pane.
> 2. Click the Trust Point Actions tab in the Information pane.
> 3. Select the crlimport option from the Command drop-down menu to import the CRL to the selected trust point.
> 4. Enter the input file name with the CRL in the bootflash:filename format, in the URL field.
> 5. Click Apply Changes to save the changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.