> # Configuring IPv6 Addressing and Enabling IPv6 Routing

> ## Detailed Steps

> To configure an IPv6 address on an interface using Device Manager, follow these steps:

> 1. Choose Interfaces > Gigabit Ethernet and iSCSI.

> You see the Gigabit Ethernet Configuration dialog box.

> 2. Click the IP Address that you want to configure and click Edit IP Address.

> You see the IP Address dialog box.

> 3. Click Create and set the IP Address/Mask field, using the IPv6 format (for example, 2001:0DB8:800:200C::417A/64).
> 4. Click Create to save these changes or click Close to discard any unsaved changes.

> To enable IPv6 routing using Device Manager, follow these steps:

> 1. Choose IP > Routing. You see the IP Routing Configuration dialog box.
> 2. Check the Routing Enabled check box.
> 3. Click Apply to save these changes or click Close to discard any unsaved changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.