> # Traffic Management Services

> In-band options are compliant with and use the RFC 2625 standards. An NMS host running the IP protocol over an Fibre Channel interface can access the switch using the IPFC functionality. If the NMS does not have a Fibre Channel HBA, in-band management can still be performed using one of the switches as an access point to the fabric .

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.