> # Zoneset Status

> Field | Description
> --- | ---
> Status | Indicates the outcome of the most recent activation/deactivation.
> Activation Time | When this entry was most recently activated. If this entry has been activated prior to the last re-initialization of the local network management system, then this value will be N/A.
> FailureCause | The reason for the failure of the zoneset activation/deactivation.
> FailedSwitch | The domain ID of the device in the fabric that has caused the Change Protocol to fail.
> Active == Local? | Indicates whether the enforced database is the same as the local database on this VSAN. If true, then they are the same. If false, then they are not the same.
> Active Zoneset | The name of the enforced IV zoneset.
> Hard Zoning | Indicates whether the hard zoning is enabled on this VSAN. Hard zoning is a mechanism by which zoning is enforced in hardware. If true, then hard zoning is enabled on this VSAN. If false, then hard zoning is not enabled on this VSAN.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.