> # Configuring DHCHAP Passwords for the Local Switch

> To configure the DHCHAP password for the local switch, follow these steps:

> 1. Expand Switches > Security, and then select FC-SP.

> You see the FC-SP configuration in the Information pane.

> 2. Click the Local Passwords tab.
> 3. Click the Create Row icon to create a new local password.

> You see the Create Local Passwords dialog box.

> 4. (Optional) Check the switches that you want to configure the same local password on.
> 5. Select the switch WNN and fill in the Password field.
> 6. Click Create to save the updated password.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.