> # Adding Authorized Port Pairs

> ## Detailed Steps

> After identifying the WWN pairs that need to be bound, add those pairs to the port security database.

> Tip Remote switch binding can be specified at the local switch. To specify the remote interfaces, you can use either the fWWN or sWWN-interface combination.

> To add authorized port pairs for port security, follow these steps:

> 1. Expand a VSAN and select Port Security in the Logical Domains pane.
> 2. Click the Config Database tab.
> 3. Click Create Row to add an authorized port pair.

> You see the Create Port Security dialog box.

> 4. Double-click the device from the available list for which you want to create the port security setting.
> 5. Double-click the port from the available list to which you want to bind the device.
> 6. Click Create to create the port security setting.
> 7. Click the Apply Changes icon to save these changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.