> # Enabling AAA Server Distribution

> ## Restrictions

> Only switches where distribution is enabled can participate in the distribution activity.

> ## Detailed Steps

> To enable RADIUS server distribution, follow these steps:

> 1. Expand Switches > Security > AAA, and then select RADIUS.

> You see the RADIUS configuration in the Information pane.

> 2. Click the CFS tab. You see the RADIUS CFS configuration.
> 3. Choose enable from the Admin drop-down list for all switches that you want to enable CFS for RADIUS.
> 4. Click Apply Changes to distribute these changes through the fabric.
> .

> To enable TACACS+ server distribution, follow these steps:

> 1. Expand Switches > Security > AAA, and then select TACACS+.

> You see the TACACS+ configuration in the Information pane.

> 2. Click the CFS tab.

> You see the TACACS+ CFS configuration.

> 3. Choose enable from the Admin drop-down list for all switches that you want to enable CFS on for TACACS+.
> 4. Click Apply Changes to distribute these changes through the fabric.
> .

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.