> # Assigning Static Port VSAN Membership

> ## Detailed Steps

> To statically assign VSAN membership for an interface, follow these steps:

> 1. Choose FC Interfaces > Physical from the Physical Attributes pane. You see the interface configuration in the Information pane.
> 2. Click the General tab.

> You see the Fibre Channel general physical information. Double-click and complete the PortVSAN field.

> 3. Click Apply Changes to save these changes, or click Undo Changes to discard any unsaved changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.