> # Enabling fctimer Distribution

> ## Detailed Steps

> To enable and distribute fctimer configuration changes using Device Manager, follow these steps:

> 1. Choose FC > Advanced > VSAN Timers.

> You see the VSANs Timer dialog box.

> 2. Fill in the timer values that you want to configure.
> 3. Click Apply to save these changes.
> 4. Select commit from the CFS drop-down menu to distribute these changes or select abort from the CFS drop-down menu to discard any unsaved changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.