# Verifying SME Tape Management Configuration

To display SME Tape management configuration information, perform one of the following tasks:

Command | Purpose
show sme cluster tape | Displays summary or detailed information about tapes.
show sme cluster tape detail | Displays information about tape cartridges.
show sme cluster tape-bkgrp | Displays information about all tape volume groups or about a specific group.

For detailed information about the fields in the output from these commands, refer to the Cisco MDS 9000 Family NX-OS Command Reference.