> # Creating an iSNS Client Profile

> ## Detailed Steps

> To create an iSNS profile, follow these steps:

> 1. Choose End Devices > iSCSI in the Physical Attributes pane.

> You see the iSCSI configuration in the Information pane.

> 2. Select the iSNS tab.
> 3. You see the iSNS profiles configured.
> 4. Click the Create Row icon.

> You see the Create iSNS Profiles dialog box.

> 5. Set the ProfileName field to the iSNS profile name that you want to create.
> 6. Set the ProfileAddr field to the IP address of the iSNS server.
> 7. Click Create to save these changes.

> To delete an iSNS profile, follow these steps:

> 1. Choose End Devices > iSCSI from the Physical Attributes pane.

> You see the iSCSI configuration in the Information pane.

> 2. Select the iSNS tab.

> You see the iSNS profiles configured.

> 3. Right-click the profile that you want to delete and click the Delete Row icon.

> To tag a profile to an interface, follow these steps:

> 1. Choose Switches > Interfaces > Gigabit Ethernet in the Physical Attributes pane.

> You see the Gigabit Ethernet configuration in the Information pane.

> 2. Click the iSNS tab.

> You see the iSNS profiles configured for these interfaces.

> 3. Set the iSNS ProfileName field to the iSNS profile name that you want to add to this interface.
> 4. Click the Apply Changes icon to save these changes.

> To untag a profile from an interface using Cisco DCNM-SAN, follow these steps:

> 1. Choose Switches > Interfaces > Gigabit Ethernet in the Physical Attributes pane.

> You see the Gigabit Ethernet Configuration in the Information pane.

> 2. Click the iSNS tab.

> You see the iSNS profiles configured for these interfaces.

> 3. Right-click the iSNS ProfileName field that you want to untag and delete the text in that field.
> 4. Click the Apply Changes icon to save these changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.