## Using FC-Redirect with CFS Regions

The Fibre Channel redirect (FC-Redirect) feature uses Cisco Fabric Services (CFS) regions to distribute the FC-Redirect configuration.

By default, the configuration is propagated to all FC-Redirect-capable switches in the fabric. CFS regions can be used to restrict the distribution of the FC-Redirect configuration.

Note Using FC-Redirect with CFS regions is an optional procedure.

To learn more about CFS regions, refer to System Management Configuration Guide, Cisco DCNM for SAN and the Cisco MDS 9000 Family NX-OS System Management Configuration Guide.