> # E Ports

> You can configure E ports in the same way you configure FCIP interfaces. The following features are also available for FCIP interfaces:
> - An FCIP interface can be a member of any VSAN
> - Trunk mode and trunk allowed VSANs
> - PortChannels
> - FSPF
> - Fibre Channel domains (fcdomains)
> - Importing and exporting the zone database from the adjacent switch
> You can configure E ports in the same way you configure FCIP interfaces. The following features are also available for FCIP interfaces:
> - An FCIP interface can be a member of any VSAN

> See the Fabric Configuration Guide,Cisco DCNM for SAN.

> - Trunk mode and trunk allowed VSANs

> See the Interfaces Configuration Guide,Cisco DCNM for SAN.

> - PortChannels
> - Multiple FCIP links can be bundled into a Fibre Channel PortChannel.
> - FCIP links and Fibre Channel links cannot be combined in one PortChannel.
>   See the Security Configuration Guide,Cisco DCNM for SAN.
> - FSPF

> See the Fabric Configuration Guide, Cisco DCNM for SAN.

> - Fibre Channel domains (fcdomains)

> See the System Management Configuration Guide, Cisco DCNM for SAN.

> - Importing and exporting the zone database from the adjacent switch

> See the System Management Configuration Guide, Cisco DCNM for SAN.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.