> # Configuring Gigabit Ethernet Interface

> ## Detailed Steps

> To configure the Gigabit Ethernet interface, follow these steps:

> 1. Expand Switches > Interfaces > Ethernet > IPS.

> You see the Gigabit Ethernet Configuration in the Information pane.

> 2. Click the IP Addresses tab.
> 3. Click Create Row.

> You see the Create Gigabit Ethernet Interface dialog box.

> 4. Select the switch on which you want to create the Gigabit Ethernet interface.
> 5. Enter the interface. For example, 2/2 for slot 2, port 2.
> 6. Enter the IPv4 address (10.1.1.100) and subnet mask (255.255.255.0).
> 7. Click Create to save these changes or click Close to discard any unsaved changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.