> # Configuring Fabric Binding

> ## Detailed Steps

> To configure fabric binding in each switch in the fabric, follow these steps:

> 1. Enable the fabric configuration feature.
> 2. Configure a list of sWWNs and their corresponding domain IDs for devices that are allowed to access the fabric.
> 3. Activate the fabric binding database.
> 4. Copy the fabric binding active database to the fabric binding config database.
> 5. Save the fabric binding configuration.
> 6. Verify the fabric binding configuration.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.