## Configuring AAA Properties

To configure AAA properties,

1. From the menu bar, choose Admin > Management Users > Remote AAA Properties.

The AAA properties configuration page appears.

2. Use the radio button to select one of the following Authentication Modes:

• Local - In this mode the authentication will authenticate with the local server.

• Radius - In this mode the authentication will authenticate against the Radius servers specified.

• TACACS+- In this mode the authentication will authenticate against the TACAS servers specified.

• Switch - In this mode the authentication will authenticate against the switches specified.

• LDAP - In this mode the authentication will authenticate against the LDAP server specified.