> # Displaying the Pending Configuration to be Distributed

> To display the RADIUS or TACACS+ global and/or server configuration stored in the temporary buffer, follow these steps:

> 1. Expand Switches > Security > AAA, and then select RADIUS or select TACACS+.
> 2. Click the CFS tab.

> You see the distribution status on the CFS tab.

> 3. Click the pending or running radio button.
> 4. Click Apply Changes to save the changes.
> 5. Click the Servers tab to view the pending or running configuration.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.