> # Enabling Time Stamp Control

> You can instruct the switch to discard packets that are outside the specified time. When enabled, this feature specifies the time range within which packets can be accepted. If the packet arrived within the range specified by this option, the packet is accepted. Otherwise, it is dropped.

> By default, time stamp control is disabled in all switches in the Cisco MDS 9000 Family. If a packet arrives within a 2000 millisecond interval (+ or –2000 msec) from the network time, that packet is accepted.

> Note The default value for packet acceptance is 2000 microseconds.If the time-stamp option is enabled, be sure to configure NTP on both switches (see the Cisco NX-OS Fundamentals Configuration Guide for more information).

> Tip Do not enable time stamp control on an FCIP interface that has tape acceleration or write acceleration configured.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.