> # Configuring AAA Properties

> To configure AAA properties,

> 1. From the menu bar, choose Admin > Management Users > Remote AAA Properties.

> The AAA properties configuration page appears.

> 2. Use the radio button to select one of the following Authentication Modes:
> - Local - In this mode the authentication will authenticate with the local server.
> - Radius - In this mode the authentication will authenticate against the Radius servers specified.
> - TACACS+- In this mode the authentication will authenticate against the TACAS servers specified.
> - Switch - In this mode the authentication will authenticate against the switches specified.
> - LDAP - In this mode the authentication will authenticate against the LDAP server specified.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.