> # Committing the Distribution

> The RADIUS or TACACS+ global and/or server configuration stored in the temporary buffer can be applied to the running configuration across all switches in the fabric (including the originating switch).

> ## Detailed Steps

> To distribute a RADIUS or TACACS+ configuration, follow these steps:

> 1. Expand Switches > Security > AAA, and then select either RADIUS or TACACS+. You see the RADIUS or TACACS+ configuration in the Information pane.
> 2. Click the CFS tab. You see the RADIUS or TACACS+ CFS configuration.
> 3. Choose commitChanges in the Config Action drop-down list for all switches that you want to enable CFS for RADIUS or TACACS+.
> 4. Click Apply Changes to distribute the changes through the fabric.
> .

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.