> # Configuring Perfect Forward Secrecy

> ## Detailed Steps

> To configure the PFS value, follow these steps:

> 1. Expand Switches > Security and then select IPSEC in the Physical Attributes pane.
> 2. Click the CryptoMap Set Entry tab.
> 3. From the drop-down list in the PFS column select the appropriate value.
> 4. Click Apply Changes to save your changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.