> # About RADIUS Server Default Configuration

> DCNM-SAN allows you to set up a default configuration that can be used for any RADIUS server that you configure the switch to communicate with. The default configuration includes:

> - Encryption type
> - Timeout value
> - Number of retransmission attempts
> - Allowing the user to specify a RADIUS server at login

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.