> # Event Destinations Addresses

> Field | Description
> --- | ---
> Address/Port | IP Address and Port to send event.
> Security Name | The SNMP parameters to be used when generating messages to be sent to this address.
> Security Model | Is used when generating SNMP messages using this entry.
> Inform Type | Trap - unacknowledged event Inform - acknowledged event.
> Inform Timeout | This expected maximum round trip time for communicating with the address.
> RetryCount | The number of retries to be attempted when a response is not received for a generated message.
> Status | Active—Port is active. NotInService—Port is out of service.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.