> # Advertising Static iSCSI Targets

> You can limit the Gigabit Ethernet interfaces through which static iSCSI targets are advertised. By default iSCSI targets are advertised on all Gigabit Ethernet interfaces, subinterfaces, PortChannel interfaces, and PortChannel subinterfaces.

> ## Detailed Steps

> To configure a specific interface that should advertise the iSCSI virtual target using Device Manager, follow these steps:

> 1. Select IP > iSCSI.

> You see the iSCSI configuration.

> 2. Click the Targets tab to display a list of existing iSCSI targets.
> 3. Right-click the iSCSI target that you want to modify and click Edit Advertised.

> You see the Advertised Interfaces dialog box.

> 4. (Optional) Right-click an interface that you want to delete and click Delete.
> 5. (Optional) Click Create to advertise on more interfaces.

> You see the Create Advertised Interfaces dialog box.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.