> # Receiving FICON Alerts

> To receive an alert to indicate any changes in the FICON configuration using Device Manager, follow these steps:

> 1. Choose FICON > VSANs.

> You see the FICON VSANs dialog box.

> 2. Check the User Alert Mode check box to receive an alert when the FICON configuration changes.
> 3. Click Apply to apply this change.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.