> # Flow Statistics

> Field | Description
> --- | ---
> Type | The matching criteria by which flows are selected to be included in the traffic which is instrumented by the ingress traffic counters.
> VsanId | The id of VSAN.
> DestId | The destination fibre channel address ID.
> SrcId | The source fibre channel address ID.
> Mask | The mask for source and destination fibre channel address ID.
> Frames | The number of received frames for the flow created by the network manager.
> Bytes | The number of received frame bytes for the flow created by the network manager.
> CreationTime | The timestamp indicating the time the row was created or modified.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.