> # iSCSI Targets

> Field | Description
> --- | ---
> Dynamically Import FC Targets | Check this option to dynamically import FC targets into the iSCSI domain. A target is not imported if it already exists in the iSCSI domain.
> iSCSI Name | The iSCSI name of the node represented by this entry.
> Dynamic | Indicates if the node represented by this entry was either automatically discovered or configured manually.
> Primary Port WWN | The FC address for this target.
> Secondary Port WWN | The optional secondary FC address for this target. This is the FC address used if the primary cannot be reached.
> LUN Map iSCSI | The configured default Logical Unit Number of this LU.
> LUN Map FC Primary | The Logical Unit Number of the remote LU for the primary port address.
> LUN Map FC Secondary | The Logical Unit Number of the remote LU for the secondary port address.
> Initiator Access All | If true, then all the initiators can access this target even those which are not in the initiator permit list of this target. If false, then only initiators which are in the permit list are allowed access to this target.
> Initiator Access List | Lists all the iSCSI nodes that are permitted to access the node represented by this entry. If AllAllowed is false and the value of List is empty, then no initiators are allowed to access this target.
> Advertised Interfaces | Lists all the interfaces on which the target could be advertised.
> Trespass Mode | The trespass mode for this node. Every iSCSI target represents one or more port(s) on the FC target. If true, the node instructs the FC node to present all LUN I/O requests to secondary port if the primary port is down.
> RevertToPrimaryPort | Indicates if it is required to revert back to primary port if the FC target comes back online.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.