> # Using Cisco DCNM-SAN Wizards

> Cisco DCNM-SAN Client provides the following wizards to facilitate common configuration tasks:

> - VSAN—Creates VSANs on multiple switches in the fabric and sets VSAN attributes including interop mode, load balancing, and FICON.
> - Zone Edit Tool—Creates zone sets, zones, and aliases. Adds members to zones and edits the zone database.
> - IVR Zone—Creates IVR zone sets, zones, and aliases. Enables IVR NAT and auto-topology. Adds members to IVR zones, and edits the IVR zone database.
> - FCoE—Creates virtual Fibre Channel (FC) interfaces and VLAN-VSAN mappings, and binds virtual FC interfaces to Ethernet interfaces or PortChannels.
> - PortChannel—Creates PortChannels from selected ISLs either manually or automatically. Sets PortChannel attributes such as channel ID and trunking mode.
> - FCIP—Creates FCIP links between Gigabit Ethernet ports. Enables Fibre Channel write acceleration and IP compression.
> - DPVM—Establishes dynamic port VSAN membership, enables autolearning, and activates the DPVM database.
> - Port Security—Prevents unauthorized access to Cisco MDS switches and reports these intrusions to the administrator.
> - iSCSI—Creates zones for iSCSI initiators and adds a VSAN to a target-allowed VSAN list.
> - NPV—Reduces the number of Fibre Channel domain IDs in SANs.
> - QoS—Sets QoS attributes for zones in the selected VSAN.
> - IP ACL—Creates ordered IP access control lists and distributes to selected switches in the fabric.
> - License Install—Facilitates download and installation of licenses in selected switches in the fabric.
> - Software Install—Verifies image compatibility and installs software images on selected switches in the fabric.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.