> # Oversubscription Ratio Restrictions

> The 48-port and 24-port 4-Gbps, and all 8-Gbps Fibre Channel switching modules support oversubscription on switches with shared rate mode configurations. By default, all 48-port and 24-port 4-Gbps, and 8-Gbps Fibre Channel switching modules have restrictions on oversubscription ratios enabled. As of Cisco SAN-OS Release 3.1(1) and NX-OS Release 4.1(1), you can disable restrictions on oversubscription ratios.

> Table 13-9 describes the bandwidth allocation for oversubscribed interfaces configured in shared mode on the 4-Gbps and 8-Gbps modules.

> Table 13-9 Bandwidth Allocation for Oversubscribed Interfaces
> Switching Module | Configured Speed | Reserved Bandwidth (Gbps) | Maximum Bandwidth (Gbps)
> --- | --- | --- | ---
> Ratios enabled | Ratios disabled
> 24-Port 8-Gbps Fibre Channel Module | Auto 8 Gbps | 0.8 | 0.8 | 8
> Auto Max 4 Gbps | 0.4 | 0.4 | 4
> Auto Max 2 Gbps | 0.2 | 0.2 | 2
> 4/44-Port 8-Gbps Host-Optimized Fibre Channel Module | 8 Gbps | 0.87 | 0.16 | 8
> Auto Max 4 Gbps | 0.436 | 0.08 | 4
> Auto Max 2 Gbps | 0.218 | 0.04 | 2
> 1 Gbps | 0.109 | 0.02 | 1
> 48-port 4-Gbps Fibre Channel switching module | Auto 4 Gbps | 0.8 | 0.09 | 4
> Auto Max 2 Gbps | 0.4 | 0.045 | 2
> 1 Gbps | 0.2 | 0.0225 | 1
> 24-port 4-Gbps Fibre Channel switching module | Auto 4 Gbps | 1 | 0.27 | 4
> Auto Max 2 Gbps | 0.5 | 0.135 | 2
> 1 Gbps | 0.25 | 0.067 | 1

> All ports in the 48-port and 24-port 4-Gbps modules can be configured to operate at 4 Gbps in shared mode even if other ports in the port group are configured in dedicated mode, regardless of available bandwidth. However, when oversubscription ratio restrictions are enabled, you may not have all shared 4-Gbps module ports operating at 4 Gbps.

> All ports in the 48-port, 32-Port, and 24-port 8-Gbps modules can be configured to operate at 8 Gbps in shared mode even if other ports in the port group are configured in dedicated mode, regardless of available bandwidth. However, when oversubscription ratio restrictions are enabled you may not have all shared 8-Gbps module ports operating at 8 Gbps.

> On the 48-port, 32-Port, and 24-port 8-Gbps modules, if you have configured one 8-Gbps dedicated port in one port group, no other ports in the same port group can be configured to operate at 8-Gbps dedicated mode. You can have any number of 8-Gbps shared and 4-Gbps dedicated or shared ports. On the 4/44-port 8-Gbps module, only one port per port group can be configured in 8-Gbps dedicated or shared mode.

> In the following example, a 24-port 4-Gbps module has oversubscription ratios enabled and three dedicated ports in one port group operating at 4-Gbps. No other ports in the same port group can be configured to operate at 4 Gbps.

> For dedicated ports, oversubscription ratio restrictions do not apply to the shared pool in port groups. So if oversubscription ratio restrictions are disabled, and you have configured three 4-Gbps dedicated ports in one port group, then you can configure all other ports in the same port group to operate at a shared rate of 4 Gbps.

> When disabling restrictions on oversubscription ratios, all ports in shared mode on 48-port and 24-port 4-Gbps or any 8-Gbps Fibre Channel switching modules must be shut down. When applying restrictions on oversubscription ratios, you must take shared ports out of service.

> Note When restrictions on oversubscription ratios are disabled, the bandwidth allocation among the shared ports is proportionate to the configured speed. If the configured speed is auto on Generation 2 modules, then bandwidth is allocated assuming a speed of 4 Gbps. For example, if you have three shared ports configured at 1, 2, and 4 Gbps, then the allocated bandwidth ratio is 1:2:4.
> As of Cisco SAN-OS Release 3.0 and NX-OS Release 4.1(1) or when restrictions on oversubscription ratios are enabled, the port bandwidths are allocated in equal proportions, regardless of port speed, so, the bandwidth allocation for the same three ports mentioned in the example would be 1:1:1.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.