> # Placing CUPs in a Zone

> ## Detailed Steps

> To place the CUP in a zone, follow these steps:

> 1. In DCNM-SAN, choose Zone > Edit Full Zoneset, and then choose Edit > Edit Default Zone Attributes to set the default zone to permit for the required VSAN.
> 2. In Device Manager, choose FC > Name Server... for the required VSAN and obtain the FICON:CUP WWN.

> Note If more than one `FICON:CUP WWN` exists in this fabric, be sure to add all the `FICON:CUP` pWWNs to the required zone.

> 3. In DCNM-SAN, choose Zone > Edit Full Zoneset and add the FICON:CUP pWWN to the zone database.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.