> # Configuring AAA Authentication for an iSCSI User

> ## Detailed Steps

> To configure AAA authentication for an iSCSI user, follow these steps:

> 1. Choose Switches > Security > AAA in the Physical Attributes pane.

> You see the AAA configuration in the Information pane.

> 2. Click the Applications tab.

> You see the AAA configuration per application.

> 3. Right-click the ServerGroup Id List field for the iSCSI application and enter the server group that you want iSCSI to use.

> Note You should use an existing server group or create a new server group before configuring it for iSCSI session authentication.

> 4. Click the Apply Changes icon to save these changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.